#
FRONT BRAKE (DISC) CONSTRUCTION [EUROPEAN (L.H.D. U.K.) SPECS.]

id0411001004c3
L8 (4SD, 5HB)
• Large diameter, ventilated disc type front brakes with a 274 mm {10.8 in} diameter and 24 mm {0.945 in} thickness have been adopted, improving braking force and fade resistance.
L8 (WGN), LF, L3 (except 18 inch wheel), MZR-CD (RF Turbo)
• Large diameter, ventilated disc type front brakes with a 283 mm {11.1 in} diameter and a 25 mm {0.984 in} thickness have been adopted, improving braking force and fade resistance.

L3 (18 inch wheel), L3 Turbo
• Large diameter, ventilated disc type front brakes with a 320 mm {12.6 in} diameter and a 25 mm {0.984 in} thickness have been adopted, improving braking force and fade resistance.