#
4-WHEEL DRIVE OUTLINE

id031800165100
• An electronic 4WD control system, which automatically optimizes traction distribution to the front and rear wheels, adopted to improve off-road mobility, handling stability, operability, fuel economy and marketability.
• Based on the input signals from each sensor, the 4WD CM determines vehicle driving and road conditions, and controls output current to the electronic control coupling (4WD solenoid) inside the rear differential. This control allows for optimal distribution of the drive torque from the engine to the rear wheels.
• A self-diagnostic function adopted for the electric 4WD control system to improve serviceability.