#
PRESSURE CONTROL SOLENOID A (LINEAR TYPE) OPERATION [FS5A-EL]

id051721004600
• By changing the electrical current value (0 A-1 A) inside the solenoid, the pressure control solenoid A adjusts the hold power of the hold pressure valve, controlling the pressure control solenoid pressure to the prescribed hydraulic pressure.

1 | Solenoid reducing pressure
2 | To pressure regulator valve
3 | Hold pressure valve

1 | Hydraulic pressure
2 | Electrical current value
3 | Pressure control solenoid pressure