#
CRUSHABLE ZONE CONSTRUCTIOIN

id091000100400
• To reduce cabin damage, the front and rear of the frame are designed to deform when incurring an impact, and effectively absorb/disperse energy from a collision.

  - In moderate collisions at the front bumper reinforcement, impact is diffused to the front side frames and front suspension members.
  - If the collision comes close to the cabin, impact is diffused to the side sills and front B frames through the torque box, reducing impact to the cabin.

1 | Collision energy
2 | Front bumper reinforcement
3 | Front side frame
4 | Front crossmember
5 | Torque box
6 | Side sill
7 | Front B-frame