#
KEYLESS ANTENNA REMOVAL/INSTALLATION

id0914z6440500

## Driver-side/passenger-side Door

1. Disconnect the negative battery cable.

2. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

3. Remove the screws.

4. Disconnect the connector, then remove the keyless antenna.

5. Install in the reverse order of removal.

## Exterior, Rear

1. Disconnect the negative battery cable.

2. Remove the screws.

3. Disconnect the connector, then remove the keyless antenna.

4. Install in the reverse order of removal.

## Interior, Front

1. Disconnect the negative battery cable.

2. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

3. Remove the bolts.

4. Disconnect the connector, then remove the keyless antenna.

5. Install in the reverse order of removal.

## Interior, Middle

1. Disconnect the negative battery cable.

2. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

3. Remove the screws.

4. Disconnect the connector, then remove the keyless antenna.

5. Install in the reverse order of removal.

## Interior, Rear [4SD]

1. Disconnect the negative battery cable.

2. Remove the screws.

3. Disconnect the connector, then remove the keyless antenna.

4. Install in the reverse order of removal.

## Interior, Rear [5HB, WGN]

### LH (LR)

1. Disconnect the negative battery cable.

2. Remove the trunk side upper trim. (LH side) (See TRUNK SIDE UPPER TRIM REMOVAL/INSTALLATION [5HB].) (See TRUNK SIDE UPPER TRIM REMOVAL/INSTALLATION [WGN].)

3. Remove the trunk side trim. (LH side) (See TRUNK SIDE TRIM REMOVAL/INSTALLATION [4SD, 5HB].) (See TRUNK SIDE TRIM REMOVAL/INSTALLATION [WGN].)

4. Remove the screws.

5. Disconnect the connector, then remove the keyless antenna.

6. Install in the reverse order of removal.

### RH (RR)

1. Disconnect the negative battery cable.

2. Remove the trunk side upper trim. (LH side) (See TRUNK SIDE UPPER TRIM REMOVAL/INSTALLATION [5HB].) (See TRUNK SIDE UPPER TRIM REMOVAL/INSTALLATION [WGN].)

3. Remove the screws.

4. Disconnect the connector, then remove the keyless antenna.

5. Install in the reverse order of removal.