#
DTC B2626, B2477

id0902i7856900

DTC B2626, B2477 | Headlight zeroset system for auto leveling control module.
--- | ---
DETECTION CONDITION | Warning • incorrect servicing of the auto leveling control module could result in electrical shock because the unit is integrated with the discharge headlight control module. Before servicing the auto leveling control module, always refer to "Discharge headlight service warnings." (See DISCHARGE HEADLIGHT SERVICE WARNINGS) Headlight zeroset for auto leveling control module is not set.
POSSIBLE CAUSE | • Headlight zeroset for auto leveling control module is not set or the setting is invalid

Diagnostic procedure

ACTION
Check connections of each sensor and the unit. Then connect WDS or equivalent and perform headlight zeroset. (See HEADLIGHT ZEROSET)