#
NOISE FILTER REMOVAL/INSTALLATION [4SD]

id092000806402

## Brake Light Noise Filter

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Nut
2 | Connector
3 | Noise filter

3. Install in the reverse order of removal.

## Rear Window Defroster Noise Filter

1. Disconnect the negative battery cable.

2. Remove the rear package trim.

3. Remove in the order indicated in the table.

1 | Bolt
2 | Connector
3 | Noise filter

4. Install in the reverse order of removal.