#
SPECIFICATION IDENTIFICATION

id000000157300
• The servicing procedure for MZR CD (RF Turbo) engines varies depending on whether the diesel particulate filter is equipped or not. To check whether the vehicle is equipped with the diesel particulate filter or not, refer to the following:
With diesel particulate filter

  • Supply pump pulley of 66mm {2.6 in} diameter.

Without diesel particulate filter

  • Supply pump pulley of 133mm {5.2 in} diameter.