- POWER WINDOW SYSTEM WIRING DIAGRAM
- FOREWORD
- POWER WINDOW SYSTEM TROUBLESHOOTING QUESTIONNAIRE
- SYMPTOM TROUBLESHOOTING CHART
- POWER WINDOW SYSTEM PRELIMINARY INSPECTION
- NO. 1 THE AUTO OPEN/CLOSE FUNCTION ON THE DRIVER'S SIDE POWER WINDOW IS INOPERATIVE
- NO. 2 THE DRIVER'S SIDE POWER WINDOW IS INOPERATIVE
- NO. 3 ALL POWER WINDOWS OTHER THAN DRIVER'S SIDE DO NOT OPERATE USING THE POWER WINDOW SUBSWITCH
- NO. 4 ALL POWER WINDOWS OTHER THAN DRIVER'S SIDE DO NOT OPERATE USING THE POWER WINDOW MAIN SWITCH
- NO. 5 ALL POWER WINDOWS ARE INOPERATIVE
- NO. 6 DOOR GLASS REVERSES EVEN THOUGH THE GLASS DOES NOT ENCOUNTER A FOREIGN OBJECT WHILE IT IS MOVING UP IN AUTOMATIC MODE
- NO. 7 ABNORMAL NOISE WHILE THE DOOR GLASS IS OPENING OR CLOSING