#
TIRE HOUSE TRIM REMOVAL/INSTALLATION

id091700802700

## 4SD

1. Remove the rear scuff plate.

2. Remove the rear seat side.

3. Remove the fastener.

4. Pull the tire house trim upward, then disengage clips A from the body, and remove the tire house trim.

5. Install in the reverse order of removal.

## 5HB, WGN

1. Remove the rear scuff plate.

2. Pull the tire house trim toward you, then disengage clip B from the body and clip A, hooks C, D from the trunk side trim.

3. Remove the tire house trim.

4. Install in the reverse order of removal.