#
SECURITY LIGHT: DTC - (WDS OR EQUIVALENT: DTC B1342)

id0902e5914100

DTC - (B1342) | PCM is defective
--- | ---
POSSIBLE CAUSE | • Defective PCM

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
- | INSPECT PCM • Clear DTCs with WDS or equivalent. • Does SST (WDS or equivalent) indicate DTC B1342 again? | Yes | Replace PCM and reprogram immobilizer system. (See IMMOBILIZER SYSTEM REPROGRAM PROCEDURE [KEYLESS ENTRY SYSTEM])
No | Connect connectors properly.