#
FRONT SUSPENSION OUTLINE

id021300100100
• A high-mount double wishbone (with double-pivoted lower arm(s)) front suspension, has been adopted.
• The front suspension design includes a link layout that provides both handling stability and riding comfort, and creates suitable camber control characteristics.
• The upper arm and lower arm(s) of the front suspension have a similar link layout to that of the conventional double wishbone suspension, except for the double-pivoted lower arm(s).
• The double-pivoted lower arm(s) allows for a small king-pin to wheel-center offset, as well as a small moment of inertia around the king-pin axis.