#
SIDE STEP MOLDING REMOVAL/INSTALLATION

id091600801800

1. Remove the fasteners.

2. Pull the side step molding outward, then disengage clips A from the body.

3. Slide the side step molding to the vehicle front and remove clips B from the side step molding.

4. Remove the side step molding.

5. Remove clips B from the body, then install it to the side step molding.

6. Install in the reverse order of removal.