#
ENGINE MOUNT OUTLINE [L3 Turbo]

id0110b3101400
• The layout of the engine mounting is pendulum type, which reduces the noise in the cabin.
• The engine supported at three points, and simplification of engine mount composition parts is attained.
• The No.3 engine mounting rubber, which is an oil-filled type, has been adopted to reduce the noise in the cabin.
• The surface of the No.3 engine joint bracket and No.1 engine-mounting rubber is made of aluminum alloy to decrease weight.

.

1 | No.3 engine joint bracket
2 | No.3 engine mount rubber
3 | No.1 engine mount rubber
4 | No.1 engine mount bracket
5 | No.4 engine mount bracket
6 | No.4 engine mount rubber