#
TURN AND HAZARD INDICATOR ALARM CONSTRUCTION/OPERATION

id092200102400

## System Wiring Diagram

1 | Instrument cluster
2 | Microcomputer
3 | Indicator buzzer
4 | CAN control circuit
5 | AND

## Operation

• The turn and hazard signal sent from the BCM via the CAN system is input to the microcomputer in the instrument cluster. The microcomputer sends an output signal to the turn indicator light and the indicator buzzer.