#
DTC 10

id070200802500

DTC 10 | Evaporator temperature sensor (present)
--- | ---
POSSIBLE CAUSE | • Evaporator temperature sensor malfunction • Climate control unit malfunction • Open or short circuit between evaporator temperature sensor and climate control unit

Diagnostic Procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Is resistance between terminals 1I and 1Q of climate control unit connector (24-pin) as indicated below? - 128 ohms-179 kilohms | Yes | Replace climate control unit.
No | Go to the next step.
2 | • Inspect evaporator temperature sensor. • Is it okay? | Yes | Repair wiring harness.
No | Replace evaporator temperature sensor.