#
AT WARNING LIGHT CONSTRUCTION/OPERATION [FS5A-EL]

id051721103000
• The AT warning light is built into the instrument cluster.
• The AT warning light illuminates when the instrument cluster receives a warning signal from the TCM via CAN communication.
• The TCM sends a warning signal to the instrument cluster via CAN communication when it detects a malfunction.

.

1 | Instrument cluster
2 | AT warning light