ENGINE CONTROL SYSTEM BLOCK DIAGRAM [L3 Turbo]

id0140b6100500

g6e140btl001

1 | MAF/IAT sensor
2 | TP sensor No.1, No.2
3 | MAP sensor
4 | CMP sensor
5 | CKP sensor
6 | ECT sensor
7 | A/F sensor
8 | HO2S
9 | Vehicle speed signal
10 | CPP switch
11 | Neutral switch
12 | Brake switch
13 | Refrigerant pressure switch (Low pressure switch, high pressure switch)
14 | Refrigerant pressure switch (Medium-pressure switch)
15 | Generator (Terminal P: starter coil)
16 | Battery
17 | BARO sensor
18 | Instrument cluster (CAN signal)
19 | APP sensor No.1, No.2
20 | Fuel pressure sensor
21 | Boost air temperature sensor
22 | Cruise control switch
23 | Ignition switch
24 | Electronic throttle control
25 | Variable swirl control
26 | Fuel injection control
27 | Fuel pump control
28 | Electronic spark advance (ESA) control
29 | Purge control
30 | EGR control
31 | A/F sensor heater control
32 | HO2S heater control
33 | A/C cut-off control
34 | Electrical fan control
35 | Generator control
36 | Starter cut-off control
37 | Variable valve timing control
38 | High pressure fuel pump control
39 | Wastegate control
40 | Fuel pump speed control
41 | Throttle actuator
42 | Throttle valve relay
43 | Variable swirl shutter valve actuator
44 | Injector driver module
45 | Fuel pump relay
46 | Ignition coil
47 | Purge solenoid valve
48 | EGR valve
49 | A/F sensor heater
50 | HO2S heater
51 | A/C relay
52 | Fan control module
53 | Generator (Terminal D: field coil)
54 | Starter relay
55 | ABS HU/CM (With ABS) (CAN signal)
56 | Instrument cluster (CAN signal)
57 | Spill valve control solenoid valve
58 | Wastegate control solenoid valve
59 | Fuel pump speed control relay