#
BRAKES FEATURES

id040000100200

Improved braking stability | • Large diameter front disc plate adopted • Large dimension front disc pad adopted • Large diameter rear disc plate adopted
Improved safety and marketability | • Dynamic stability control (DSC) has been adopted • Electrical brake assist control has been adopted (with DSC) • Intrusion-minimizing brake pedal adopted
Improved serviceability | • Integrated DSC HU/CM adopted • Combine sensor adopted • CAN communication function adopted • Enhanced malfunction diagnosis system for use with WDS or equivalent
Improved Reliability | • Integrated construction of the hydraulic unit (HU) and control module (CM) has been adopted for the ABS (ABS/TCS) HU/CM and DSC HU/CM • DSC HU/CM with built-in brake fluid pressure sensor has been adopted.
Modifications to match vehicle characteristics | • Vacuum pump and vacuum switch added (MZR-CD (RF Turbo)) • DSC HU/CM uses the forward-G signal from combine sensor to control DSC (4WD)