#
TCS OFF SWITCH REMOVAL/INSTALLATION

id041400201700

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | TCS off switch (SeeTCS Off Switch Removal Note)
2 | Connector

3. Install in the reverse order of removal.

## TCS Off Switch Removal Note

1. Insert your hand from the lower side of the dashboard and squeeze the tabs of the TCS off switch.

2. Pull the TCS off switch forward to remove it.