#
TRIPLE CONE SYNCHRONIZER MECHANISM STRUCTURE [G35M-R]

id0515b1101800

## Features

• A triple cone synchronizer mechanism is used for the 1st and 2nd gears.
• The triple cone synchronizer mechanism is a compact device capable of heavy duty meshing.
• The synchronizer mechanism reduces meshing time and improves operation.
• The triple cone synchro mechanism includes a synchronizer ring, double cone, and an inner cone.
• The inner part of the inner cone is used as a friction surface.

Structure

.

1 | 1st gear
2 | Inner cone
3 | Double cone
4 | Synchronizer ring
5 | Clutch hub
6 | Clutch hub sleeve
7 | Synchronizer ring
8 | Double cone
9 | Inner cone
10 | 2nd gear