#
NO.4 CASSETTE TAPE PLAYER EJECT THE CASSETTE TAPE IMMEDIATELY

id0903a1870500

4 | Cassette tape player ejects the cassette tape immediately./00:Er04, 00:Er10
TROUBLESHOOTING HINTS • Cassette tape is malfunctioning. • Cassette tape player is malfunctioning.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Replace with the cassette tape known to be good. • Does the cassette tape player eject the cassette tape immediately? | Yes | Replace the cassette tape player.
No | The cassette tape player is normal. Explain to the customer that the cassette tape is malfunctioning (e.g.,slack, broken, etc.).