#
NO.2 MIL ILLUMINATES [MZR-CD (RF Turbo)]

id0103f1800800

2 | MIL ILLUMINATES
--- | ---
DESCRIPTION | • MIL illuminates incorrectly.
POSSIBLE CAUSE | • PCM illuminates for emission-related concern (DTC is stored in PCM) • Instrument cluster malfunction Note • If MIL blinks at a steady rate, a misfire condition could possibly exist.

Diagnostic procedure

STEP | INSPECTION | RESULTS | ACTION
--- | --- | --- | ---
1 | Connect the WDS or equivalent to the DLC-2. Turn the engine switch to the ON position. Retrieve any DTCs. Are any DTCs displayed? | Yes | DTC is displayed: • Go to the appropriate DTC test. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | No DTC is displayed: • Inspect the instrument cluster operation.
2 | Verify test results. • If normal, return to the diagnostic index to service any additional symptoms. (See SYMPTOM DIAGNOSTIC INDEX [MZR-CD (RF Turbo)].) • If the malfunction remains, inspect the related Service Information and perform repair or diagnosis. - If the vehicle is repaired, troubleshooting completed. - If the vehicle is not repaired or additional diagnostic information is not available, reprogram the PCM if later calibration is available. Retest.