#
VALVE MECHANISM CONSTRUCTION [MZR-CD (RF Turbo)]

id0110f1117200
• An OHC type valve system has been adopted and consists of 2 intake valves and 2 exhaust valves per cylinder total of 16 valves operated by one camshaft via the rocker arm and rocker bridge.

.

1 | Timing belt
2 | Camshaft pulley
3 | Water pump pulley
4 | Timing belt auto tensioner
5 | Tensioner pulley
6 | Camshaft
7 | Rocker arm
8 | Rocker bridge
9 | Supply pump pulley
10 | Idler pulley
11 | Timing belt pulley