#
CONTROL VALVE BODY OUTLINE [JA5AX-EL]

id051705110100
• The control valve body is composed of four bodies: the sub lower body, lower body, internal body, and the upper body.
• To minimize the component in the control valve body, clutch engagement is electronically controlled, hydraulic circuits were simplified and the valve types reduced.

.

1 | Fail-safe valve
2 | Shift valve B
3 | Shift valve A
4 | TCC control valve
5 | Neutral shift valve
6 | Manual valve
7 | Pilot valve
8 | Accumulator switch valve
9 | Neutral control valve
10 | Reduction timing valve
11 | Reduction reducing valve
12 | Shift valve C
13 | Low clutch accumulator
14 | High clutch accumulator
15 | Line pressure relief valve
16 | Pressure regulator valve
17 | Accumulator control valve B
18 | Throttle accumulator B
19 | Pressure modifier valve
20 | Modifier accumulator
21 | Torque converter pressure regulator valve
22 | Throttle accumulator A
23 | Accumulator control valve A
24 | Throttle accumulator C
25 | Accumulator control valve C