#
EXTERIOR OPEN/CLOSE FUNCTION BLOCK DIAGRAM

id091200102200

With Advanced Keyless System

.

1 | Transmitter
2 | Request switch (driver's side)
3 | Keyless receiver
4 | Keyless control module
5 | Door switch
6 | Push switch / key reminder switch
7 | • Trun compartment light switch (4SD) • Cargo compartment light switch (5HB, WGN)
8 | Power window main switch
9 | Input signal
10 | Control signal
11 | Power window subswitch (RF)
12 | Power window subswitch (LR)
13 | Power window subswitch (RR)
14 | Power window motor (LF)
15 | Power window motor (RF)
16 | Power window motor (LR)
17 | Power window motor (RR)

With Keyless Entry System

.

1 | Transmitter
2 | Keyless receiver
3 | Door switch
4 | key reminder switch
5 | • Trun compartment light switch (4SD) • Cargo compartment light switch (5HB, WGN)
6 | Input signal
7 | Control signal
8 | Power window main switch
9 | Power window subswitch (RF)
10 | Power window subswitch (LR)
11 | Power window subswitch (RR)
12 | Power window motor (LF)
13 | Power window motor (RF)
14 | Power window motor (LR)
15 | Power window motor (RR)