#
NO.11 TRACK CHANGE IS INOPERATIVE.

id0903a1806900

11 | Track change is inoperative./03:Er02, 06:Er02, 10:Er02, 22:Er02
TROUBLESHOOTING HINTS • Audio unit is malfunctioning. • Defective CD. (e.g., cracked, badly bent, rough edges, scratch, dirty CD, condensation). • Non-conventional discs. (e.g., 8cm (3 in) CD, 8cm (3 in) disc adapter, heart-shaped disc, octagonal disc) • Center panel is malfunctioning. • MP3 applicable CD player is malfunctioning.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Replace the Cd known to be good. • Does the Cd player change the track? | Yes | Explain to the customer that the defective CD or non-conventional disc cannot be use.
No | Go to the next step.
2 | • Inspect the center panel installation. • Does the Cd player change the track number on the display when pressing the track up or down button? | Yes | Replace the audio unit.
No | Go to the "No.1 Audio panel switch inspection" in this section. Replace the center panel as necessary.