#
ELECTRONIC CONTROL COUPLING CONSTRUCTION

id031800166500
• The electronic control coupling basically consists of an electromagnetic clutch, a cam mechanism and a torque transmission system.
• The electromagnetic clutch consists of a 4WD solenoid (electromagnetic coil), rear-housing that forms a magnetic path, pilot clutch, and armature. The cam mechanism consists of a pilot cam, balls, and main cam. The torque transmission system consists of a main clutch and hydraulic oil (ATF).

.

1 | Front wheel side
2 | Rear wheel side
3 | Torque transmission system
4 | Electromagnetic clutch
5 | Rear housing
6 | 4WD solenoid (Electromagnetic coil)
7 | Cam mechanism
8 | Ball
9 | Main clutch
10 | Main cam
11 | Armature
12 | Pilot clutch
13 | Pilot cam