#
FUEL PUMP UNIT FUNCTION [L8, LF, L3]

id0114b1101400
• Due to the adoption of the mechanical returnless fuel system.
• The fuel pump unit, except for the fuel gauge sender unit, is integrated.
• To prevent decreased engine output from a lack of fuel supply when the vehicle is turning, the fuel pump has been designed so the fuel supply always remains constant in the fuel reservoir cup.
• Fuel stored in the fuel reservoir cup is supplied from two lines: the check valve (one-way) and the jet pump.