#
DRIVE BELT CONSTRUCTION [L3 Turbo]

id0110b3102500
• A serpentine type drive belt with a V-ribbed belt to drive the supplemental units has been adopted. This shortens the engine length and improves serviceability.
• A front drive belt auto tensioner with an embedded coil spring has been adopted to automatically maintain the optimal drive belt tension.

.

1 | P/S oil pump pulley
2 | Drive belt
3 | Idler pulley
4 | Generator pulley
5 | Front drive belt auto tensioner
6 | Crankshaft pulley
7 | A/C compressor pulley
8 | Water pump pulley