#
REAR STABILIZER REMOVAL/INSTALLATION [2WD]

id0214008005a1

1. Remove the rear auto leveling sensor.

(See REAR AUTO LEVELING SENSOR REMOVAL/INSTALLATION [2WD].) (See REAR AUTO LEVELING SENSOR REMOVAL/INSTALLATION [4WD].)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

4. Adjust the headlight zeroset.

(See HEADLIGHT ZEROSET.)

.

1 | Stabilizer control link
2 | Stabilizer bracket
3 | Bushing
4 | Rear stabilizer