ENGINE CONTROL SYSTEM OUTLINE [MZR-CD (RF Turbo)]

id0140f1100100

Features

Improved emission gas purification | • Intake shutter valve control adopted • Fuel injection control changed • Diesel particulate filter regeneration control adopted • EGR control adopted
Wiring harness simplification | • Controller area network (CAN) adopted
Improved drivability | • Cruise control adopted

Specification

Item | Specification
--- | ---
IAT sensor (Inside MAF) | Thermistor
MAF sensor | Hot-wire
IAT sensor No.2 | Thermistor
Intake shutter valve position sensor | Hall element type
Boost sensor | Piezoelectric element
ECT sensor | Thermistor
CMP sensor | Magneto resistance element
CKP sensor | Magneto resistance element
APP sensor | Hall element type
EGR valve position sensor | Potentiometer
Exhaust gas temperature sensor (Lower) | Thermistor
Exhaust gas temperature sensor (Middle) | Thermistor
Exhaust gas temperature sensor (Upper) | Thermistor
Exhaust gas pressure sensor | Semiconductor type
A/F sensor | Zirconia element
BARO sensor (built into PCM) | Piezoelectric element
Fuel temperature sensor | Thermistor
Fuel pressure sensor | Piezoelectric element
Exhaust gas pressure correction temperature sensor | Thermistor
Neutral switch | ON/OFF
Clutch switch | ON/OFF
PSP switch | ON/OFF