#
DTC TABLE [DISCHARGE HEADLIGHT]

id0902b2837000
• DTCs are common for present and past malfunction diagnosis.

DTC | Description | Page
--- | --- | ---
B2386 | Discharge headlight illumination malfunction. | (See DTC B2386)
B2387 | Ignitor circuit malfunction. | (See DTC B2387)
B2388 | Discharge headlight operating voltage out of range. | (See DTC B2388)
B2389 | Discharge headlight illumination malfunction. | (See DTC B2389)
B2391 | Discharge headlight input resistance too high. | (See DTC B2391)
B2392 | Discharge headlight input voltage high. | (See DTC B2392)
B2393 | Discharge headlight control module output circuit malfunction. | (See DTC B2393)