#
ENGINE FRONT COVER [L3]

id0110a11191a4

## Structure

• The engine front cover is made of aluminum alloy, and is integrated with the No.3 engine mounting bracket to improve noise absorption and weight reduction.
• The bolt hole for crankshaft pulley positioning, the service hole for unlocking the chain adjuster ratchet, and the service hole for securing the tensioner arm when loosening the timing chain are on the engine front cover.
• The oil line and the integrated oil filter are on the engine front cover.

.

1 | No.3 engine mount bracket
2 | Oil filter
3 | Front view
4 | Service hole for tensioner arm fixation
5 | Service hole for chain tensioner lock release
6 | Bolt hole crankshaft pulley positioning
7 | No.3 engine mount bracket
8 | Back view
9 | Oil filter
10 | Oil passage to oil control valve (OCV)