#
REAR BRAKE (DISC) CONSTRUCTION

id041100100300
L8, LF, L3 (except 18 inch wheel), MZR-CD (RF Turbo)
• Large diameter, solid-disc type rear brakes with a 280 mm {11.0 in} diameter and 10 mm {0.39 in} thickness have been adopted, improving braking force and fade resistance.

L3 (18 inch wheel), L3 Turbo
• Large diameter, solid-disc type rear brakes with a 314 mm {12.4 in} diameter and 11 mm {0.43 in} thickness have been adopted, improving braking force and fade resistance.