#
POWER WINDOW SYSTEM OUTLINE

id091200006400

## Features

• The following functions have been adopted for all windows.

  - Manual open/close function
  - Auto-open/close function
  - Auto reverse pinch protection function
  - Two-step down function
  - Ignition off timer function
  - Fail-safe function

• A power-cut function that permits disabling the operation of all window switches except driver's window from the driver's seat has been adopted.
• The P/W CM (power window control module) inside the power window switch, which detects the door glass movement distance and direction based on pulse signals of the power window motor, controls these functions.