#
BOOST AIR TEMPERATURE SENSOR CONSTRUCTION/OPERATION [L3 Turbo]

id0140b6104400
• The boost air temperature sensor is built into the MAP sensor.

1 | MAP/boost air temperature sensor
2 | Boost air temperature sensor characteristic
3 | Large
4 | Resistance
5 | Small
6 | Low
7 | Boost air temperature
8 | High

• The boost air temperature sensor is a thermistor type, the resistance changes according to the intake air temperature.
• The resistance decreases if the intake air temperature increases and conversely increases if the intake air temperature decreases.