#
INJECTOR DRIVER MODULE FUNCTION [L3 Turbo]

id0140b6105100
• An injector driver module which can provide high voltage has been adopted to drive the fuel injector which corresponds to a base high fuel pressure of 3-11.5 Mpa {31-117 kgf/cm 2, 435-1667 psi}.
• The injector driver module is located on the side frame under the battery tray.
• The injector driver module provides the boosted voltage to the fuel injector according to the fuel injection signal from the PCM.