ENGINE CONTROL SYSTEM DIAGRAM [L8, LF, L3]

id0140a5100300

d6e116at3005

1 | Ignition coil
2 | APP sensor
3 | VAD shutter valve (L3)
4 | Air cleaner
5 | MAF sensor
6 | VAD shutter valve actuator (L3)
7 | VAD solenoid valve (L3)
8 | Vacuum chamber (L3)
9 | VAD check valve (one-way) (L3)
10 | Purge solenoid valve
11 | Throttle actuator
12 | TP sensor
13 | MAP sensor
14 | Variable intake air control solenoid valve (LF, L3)
15 | Variable tumble solenoid valve
16 | Variable intake air shutter valve actuator (LF, L3)
17 | Variable intake air shutter valve (LF, L3)
18 | Variable tumble shutter valve actuator
19 | Variable tumble shutter valve
20 | Fuel injector
21 | OCV (LF, L3)
22 | CMP sensor
23 | EGR valve
24 | Knock sensor
25 | ECT sensor
26 | PCV valve
27 | CKP sensor
28 | A/F sensor
29 | HO2S
30 | Charcoal canister
31 | Check valve (two-way)
32 | Pressure regulator
33 | Fuel filter (high pressure)
34 | Fuel pump
35 | Fuel filter (low pressure)
36 | Fuel tank
37 | Rollover valve
38 | Jet pump (transfer)
39 | To PCM