#
REMOTE HANDLE LEVER REMOVAL/INSTALLATION

id091300800600

## 4SD

1. To remove the remote wire, remove the trunk side trim.

2. Remove in the order indicated in the table.

1 | Remote handle lever
2 | Remote wire
3 | Remote catch

3. Install in the reverse order of removal.

## 5HB, WGN

1. To remove the remote wire, remove the trunk side upper trim and trunk side lower trim.

2. Remove in the order indicated in the table.

1 | Remote handle lever
2 | Cover
3 | Remote wire

3. Install in the reverse order of removal.