#
COIL ANTENNA REMOVAL/INSTALLATION [KEYLESS ENTRY SYSTEM]

id0914b3804900

  Note

  • Do not remove the coil antenna unless you are replacing it.
  • When only the coil antenna is replaced, the immobilizer system reprogram procedure is not necessary.

1. Disconnect the negative battery cable.

2. Remove the column cover.

3. Remove in the order indicated in the table.

1 | Connector
2 | Coil antenna

4. Install in the reverse order of removal.