#
SLOPE MODE CONTROL OUTLINE [JA5AX-EL]

id051705108500
• Climbing and the appropriate gear is determined by engine load and the vehicle acceleration.

## Slope Mode Control Block Diagram

.

1 | Starter
2 | TR switch
3 | Down switch
4 | Up switch
5 | M range switch
6 | TFT sensor
7 | PCM
8 | CAN
9 | Input
10 | Throttle position signal
Engine speed signal
Engine torque signal
11 | TCM
12 | Throttle opening angle
13 | Shift diagram
14 | Vehicle speed
15 | VSS
16 | Shift solenoid A
17 | Shift solenoid B
18 | Shift solenoid C

### When climbing hill

  • When the hill is steeper than a certain grade, unnecessary up shift is prevented by holding an appropriate gear.