#
BODY CONTROL MODULE (BCM) WIRING DIAGRAM

id094000101600

1 | • Trunk compartment light switch(4SD) • Cargo compartment light switch (5HB, WGN)
2 | Driver's side door key cylinder switch
3 | Trunk lid key cylinder switch
4 | Driver's side door lock-link switch
5 | Rear left side door lock-link switch
6 | Rear right side door lock-link switch
7 | Passenger's side door lock-link switch
8 | Hazard warning switch
9 | Bonnet switch
10 | Key reminder switch
11 | Courtesy light
12 | Map light
13 | Turn switch
14 | Ignition key cylinder illumination
15 | Security light
16 | Door ajar warning light
17 | Instrument cluster
18 | Door switch (driver's side)
19 | Door switch (rear, left)
20 | Door switch (rear, right)
21 | Door switch (passenger's side)
22 | Door lock actuator (without double locking system)
23 | Door lock actuator (with double locking system)
24 | • Trunk lid opener (4SD) • Liftgate lock actuator (5HB, WGN)
25 | Front turn light (RH)
26 | Front turn light (LH)
27 | Rear turn light (RH)
28 | Rear turn light (LH)
29 | To power window main switch
30 | • Keyless control module (with advanced keyless system) • Keyless receiver (with keyless entry system)
31 | BCM

1 | • DSC HU/CM (with DSC) • ABS HU/CM (with ABS)
2 | Fuel gauge sender unit
3 | To brake light switch
4 | To tail light
5 | Rear washer motor
6 | Rear washer switch
7 | Rear wiper motor
8 | Rear wiper switch
9 | Theft-deterrent siren
10 | Horn relay
11 | Horn
12 | Horn switch
13 | To DLC-2
14 | To back-up light switch
15 | To audio system
16 | To headlight leveling switch
17 | Intruder sensor (front)
18 | Intruder sensor (rear) (WGN only)
19 | BCM