#
JOINT SHAFT ASSEMBLY [L3 Turbo]

id0313008011b5

1. Assemble in the order indicated in the table.

1 | Bracket
2 | Bearing (See Bearing Assembly Note)
3 | Snap ring
4 | Joint shaft (See Joint Shaft Assembly Note)
5 | Dust seal (See Dust Seal Assembly Note)
6 | Snap ring

## Bearing Assembly Note

1. Install the new bearing to the bracket.

  Note

  • When the bearing is not installed to the bracket by hand, install it using the SST.

## Joint Shaft Assembly Note

1. Install the joint shaft using a press and the SST.

## Dust Seal Assembly Note

1. Apply grease to the new dust seal lip.

2. Install the new dust seal using a press and the SST.