#
INSTRUMENT CLUSTER STRUCTURAL VIEW

id092200101200

## Meter And Gauge

.

1 | Tachometer
2 | Speedometer
3 | Water temperature gauge
4 | Fuel gauge
5 | Tripmeter switch
6 | Odometer/tripmeter

## Warning And Indicator Light

×: Applicable

No. | Warning and indicator light | Input signal source | CAN system | Note
--- | --- | --- | --- | ---
1 | Cruise main indicator light | PCM | × | With cruise control system
2 | Washer fluid level warning light | Washer fluid level sensor | - | -
3 | Cruise set indicator light | PCM | × | With cruise control system
4 | Turn indicator light | BCM | × | -
5 | ABS warning light | • DSC HU/CM • ABS/TCS HU/CM • ABS HU/CM | × | -
6 | Front fog indicator light | Front fog light relay | - | -
7 | AT warning light | PCM | × | ATX
8 | Diesel particulate filter warning light | PCM | × | MZR-CD (RF turbo)
9 | High-beam indicator light | BCM | × | -
10 | Rear fog indicator light | Rear fog light relay | - | -
11 | DSC/TCS indicator light | • DSC HU/CM • ABS/TCS HU/CM | × | With DSC or ABS/TCS
12 | TNS indicator light | TNS relay | - | -
13 | TCS OFF light | ABS/TCS HU/CM | × | With ABS/TCS
14 | 4WD indicator light | 4WD control module | × | 4WD
15 | Glow indicator light | PCM | × | MZR-CD (RF turbo)
16 | DSC OFF light | DSC HU/CM | × | With DSC
17 | Fuel level warning light | Fuel gauge sender unit | - | -
18 | Selector indicator light | PCM | × | ATX
19 | MIL | PCM | × | -
20 | Brake system warning light | • DSC HU/CM • ABS/TCS HU/CM • ABS HU/CM | × | -
21 | Generator warning light | PCM | × | -
22 | Oil pressure warning light | Oil pressure switch | - | -
23 | Air bag system warning light | SAS control module | - | -
24 | Door ajar warning light | BCM | × | -
25 | Seat belt warning light | Buckle switch | - | -
26 | Security light | - | - | -
27 | • Keyless indicator light (green) • Keyless warning light (red) | Keyless control module | × | With advanced keyless system