#
SECONDARY SHAFT (NO.2) COMPONENTS DISASSEMBLY

D6E051517040109

1. Disassemble in the order shown in the figure.

1 | Snap ring
2 | Rear bearing (See Rear Bearing and 6th Gear Disassembly Note.)
3 | 6th gear (See Rear Bearing and 6th Gear Disassembly Note.)
4 | 6th needle bearing
5 | Spacer
6 | 6th synchronizer ring
7 | Snap ring
8 | 5th/6th clutch hub component (See 5th Gear and 5th/6th Clutch Hub Disassembly Note.)
9 | Clutch hub sleeve
10 | Steel ball
11 | Spring
12 | Synchronizer key
13 | Clutch hub
14 | 5th synchronizer ring
15 | 5th gear (See 5th Gear and 5th/6th Clutch Hub Disassembly Note.)
16 | Spacer
17 | 5th needle bearing
18 | Spacer
19 | Snap ring
20 | Reverse clutch hub component (See Reverse Gear and Reverse Clutch Hub Disassembly Note.)
21 | Clutch hub sleeve
22 | Synchronizer key
23 | Spring
24 | Clutch hub
25 | Reverse synchronizer ring
26 | Reverse gear (See Reverse Gear and Reverse Clutch Hub Disassembly Note.)
27 | Reverse needle bearing
28 | Front bearing (See Front Bearing Disassembly Note.)
29 | Secondary shaft (No.2)

## Rear Bearing and 6th Gear Disassembly Note

1. Using the SST and a press, remove the 6th gear and rear bearing at the same time.

## 5th Gear and 5th/6th Clutch Hub Disassembly Note

1. Using the SST and a press, remove the 5th gear and 5th/6th clutch hub at the same time.

## Reverse Gear and Reverse Clutch Hub Disassembly Note

1. Using the SST and a press, remove the reverse gear and reverse clutch hub at the same time.

## Front Bearing Disassembly Note

1. Using the SST and a press, remove the front bearing.