#
SLOPE MODE CONTROL OPERATION [FS5A-EL]

id051721108400

## Climbing hill

• When the hill is steeper than a specified grade, unnecessary shift up is prevented by holding an appropriate shift gear.

## Descending hill

• When the descent is steeper than a specified grade and the brake switch is depressed, use of the brake pedal is reduced by shifting from 5GR to 4GR or from 4GR to 3GR and applying the engine brake effectively.