#
REAR SEAT REMOVAL/INSTALLATION [EXCEPT WGN (4WD)]

id0913008004a3

## 4SD

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

1 | Rear seat cushion
2 | Rear side seat
3 | Rear seat back

## 5HB, WGN (2WD)

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

1 | Remote wire (See Remote wire removal note)
2 | Rear seat (See Rear seat removal note)

### Remote wire removal note

1. Turn over the trunk floor mat.

2. Remove the case.

3. Remove the remote wire.

### Rear seat removal note

1. Remove the front hinge installation bolts.

2. Lift the rear seat cushion, then remove the rear hinge installation bolts.