#
INTRUDER SENSOR OUTLINE

id0914b5870100
• The intruder sensor is located in center part of the roof on sliding sunroof-equipped vehicles or the forward part of the roof on sliding sunroof non-equipped vehicles.
• The intruder sensor detects movement in the vehicle by radio waves and sends the detection signal to the theft-deterrent control module.
• An intruder sensor cut-off switch has been installed on the keyless entry system transmitter. If the intruder sensor cut-off switch is on while the theft-deterrent system is pre-armed, intruder sensor radio wave output is cut, and movement detection is stopped.

.

1 | Intruder sensor (without sliding sunroof)
2 | Intruder sensor (with sliding sunroof)
3 | Rear intruder sensor (WGN)
4 | Transmitter
5 | Intruder sensor cut-off switch