#
OUTSIDE MIRROR SYSTEM WIRING DIAGRAM

id091200007200

Vehicle without retract/return

.

1 | Power outside mirror switch
2 | Power outside mirror (left side)
3 | Power outside mirror (right side)
4 | Left
5 | Right
6 | Up
7 | Down
8 | Up switch
9 | Down switch
10 | Left switch
11 | Right switch
12 | To power window main switch
13 | Left
14 | Right

Vehicle with retract/return

.

1 | Power outside mirror switch
2 | Power outside mirror (left side)
3 | Power outside mirror (right side)
4 | Left
5 | Right
6 | Up
7 | Down
8 | Up switch
9 | Down switch
10 | Left switch
11 | Right switch
12 | Retract/return motor (left side)
13 | Retract/return motor (right side)
14 | Return
15 | Retract
16 | To power window main switch
17 | Left switch
18 | Right switch
19 | Return switch
20 | Retract switch